{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["工程量清单"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"工程量清单","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"merged":[[0,0,0,6],[26,0,26,6],[27,0,27,6]],"flags":["formulas_cached_only"]}
["工程量清单"]
["序号","项  目  名  称","单位","数量","单价（元）","合价（元）","备注"]
[1,"基本服务项目"]
[1.1,"进出坞费","项",1,null,null,"包括进坞、出坞"]
[1.2,"住坞费   ","天",10,null,null,"据实结算"]
[1.2999999999999998,"消防、安全巡视值班费","天",10,null,null,"据实结算"]
[1.3999999999999997,"防污费","天",10,null,null,"据实结算"]
[1.4999999999999996,"电费（指住坞期间船上接电用量，度数以船坞电表为准）","度",2000,null,null,"据实结算"]
[1.5999999999999994,"围油栏费","项",1]
[2,"工程项目"]
[2.1,"坞修工程勘测费","项",1]
[2.2,"船舶搭拆临时电、水源","项",1]
[2.3000000000000003,"船舶带缆费","项",1]
[2.4000000000000004,"左右舵拆装、密封更换","扇",2,null,null,"含密封"]
[2.5000000000000004,"左右舵轴间隙检测","项",1]
[2.6000000000000005,"左右螺旋桨拆装、密封更换","只",2,null,null,"含密封"]
[2.7000000000000006,"左右尾轴间隙检测","项",1]
[2.8000000000000007,"海底进水格栅拆装焊接，清洁、油漆","个",2]
[2.900000000000001,"海底阀、滤网拆解、清洁、研磨、密性试验","套",2]
["2.10","主甲板以下黑杆除锈油漆（花铲除锈、拉毛）","㎡",56,null,null,"含油漆"]
["2.11","主甲板黑杆以下到满载水线以上除锈油漆（风沙除锈）","㎡",298,null,null,"含油漆"]
["2.12","满载水线以下除锈油漆（风沙除锈）","㎡",1448,null,null,"含油漆"]
["2.13","加装桅杆收放器（设备、钢材、钢丝绳、工时费、耗材等）","套",1]
["2.14","资料费","项",1]
["2.15","暂列金额","项",1]
[3,"工程总价（1+2）"]
["备注：1、工程单价为全费用单价，是完成工程量清单中一个质量合格的规定计量单位项目所需的人工费、材料费、机械使用费、管理费、利润、组织及技术措施费、规费、税金，以及合同明示或暗示的所有责任、义务和一般风险因素等。"]
["2、天：指日历天。"]